





Using conservation of momentum. Since mass cancels, the new velocities are just ratios of the mass to the first velocity. mv0 = (am + bm + cm ….)v1

  
  
Torque acts as a friction here, countering the force of gravity of the sphere rolling down. Note that the water in the sphere does not rotate, so when considering the moment of inertia, we use the inertia of the empty shell. So the force of the sphere rolling down, 2MA is the result of the frictional torque, 2/3 MA subtracted from the force of gravity, 2Mgsin@.






If momentum is conserved, then the velocity of the center of mass never changes. More on this in CCof Physics.



We cannot use ½ Iw^2 here. The conserved angular momentum must be used instead.   
  
   



Torques and forced need to be balanced. As the apparatus clearly does not rotate and does not slide in any direction, we must balance both the two torques (from friction and the applied force) and the two forces (same).

For the two torques, we have from friction .2f and from applied force .1F. Since these two act in opposite directions, they need to be equal : .2f = F

The two horizontal forces also cancel, this is from the applied force’s horizontal component Fcos0 and the force of friction f.

Fcos0 = f;

Solving for 0 we get 0 = 60.